enable device access via elogind

--- a/host/libhackrf/53-hackrf.rules.in
+++ b/host/libhackrf/53-hackrf.rules.in
@@ -1,13 +1,13 @@
 # HackRF Jawbreaker
-ATTR{idVendor}=="1d50", ATTR{idProduct}=="604b", SYMLINK+="hackrf-jawbreaker-%k", MODE="660", GROUP="@HACKRF_GROUP@"
+ATTR{idVendor}=="1d50", ATTR{idProduct}=="604b", SYMLINK+="hackrf-jawbreaker-%k", MODE="660", GROUP="@HACKRF_GROUP@", TAG+="uaccess"
 # HackRF One
-ATTR{idVendor}=="1d50", ATTR{idProduct}=="6089", SYMLINK+="hackrf-one-%k", MODE="660", GROUP="@HACKRF_GROUP@"
+ATTR{idVendor}=="1d50", ATTR{idProduct}=="6089", SYMLINK+="hackrf-one-%k", MODE="660", GROUP="@HACKRF_GROUP@", TAG+="uaccess"
 # rad1o
-ATTR{idVendor}=="1d50", ATTR{idProduct}=="cc15", SYMLINK+="rad1o-%k", MODE="660", GROUP="@HACKRF_GROUP@"
+ATTR{idVendor}=="1d50", ATTR{idProduct}=="cc15", SYMLINK+="rad1o-%k", MODE="660", GROUP="@HACKRF_GROUP@", TAG+="uaccess"
 # NXP Semiconductors DFU mode (HackRF and rad1o)
-ATTR{idVendor}=="1fc9", ATTR{idProduct}=="000c", SYMLINK+="nxp-dfu-%k", MODE="660", GROUP="@HACKRF_GROUP@"
+ATTR{idVendor}=="1fc9", ATTR{idProduct}=="000c", SYMLINK+="nxp-dfu-%k", MODE="660", GROUP="@HACKRF_GROUP@", TAG+="uaccess"
 # rad1o "full flash" mode
-KERNEL=="sd?", SUBSYSTEM=="block", ENV{ID_VENDOR_ID}=="1fc9", ENV{ID_MODEL_ID}=="0042", SYMLINK+="rad1o-flash-%k", MODE="660", GROUP="@HACKRF_GROUP@"
+KERNEL=="sd?", SUBSYSTEM=="block", ENV{ID_VENDOR_ID}=="1fc9", ENV{ID_MODEL_ID}=="0042", SYMLINK+="rad1o-flash-%k", MODE="660", GROUP="@HACKRF_GROUP@", TAG+="uaccess"
 # rad1o flash disk
-KERNEL=="sd?", SUBSYSTEM=="block", ENV{ID_VENDOR_ID}=="1fc9", ENV{ID_MODEL_ID}=="0082", SYMLINK+="rad1o-msc-%k", MODE="660", GROUP="@HACKRF_GROUP@"
+KERNEL=="sd?", SUBSYSTEM=="block", ENV{ID_VENDOR_ID}=="1fc9", ENV{ID_MODEL_ID}=="0082", SYMLINK+="rad1o-msc-%k", MODE="660", GROUP="@HACKRF_GROUP@", TAG+="uaccess"
 #
